===========================================
|HeadAC3he's known issues by Dark Avenger |
-------------------------------------------
|website: http://darkav.de.vu             |
|  email: darkav@gmx.net                  |
-------------------------------------------


HeadAC3he core:

- Make sure destination/temporary size is below 4GB for FAT32.

- for 6ch decodes you probably need NTFS in float mode...

- no corrupt ac3 handling
  (properly ripped, there shouldn't be corrupt ac3s anyway; try to rip at
  low system load and demux with dvd2avi if you experience crc errors in ac3/
  azid crashes or says bad sync frame.)

- implemented Ligh's boost function as post filter for all modes except hybrid mode,
  for latter it is a pre-filter due its restrictions, so for hybrid mode you probably
  need a higher boost value to get the same effect. Unfortunately this value is
  dependant on the ac3.


AZID:

- if want to downmix to mono (why the heck?) LFE isn't downmixed.

- if you output more than 2 channels, don't forget to change input gain to 0db for the
  now seperated channels otherwise you may not get what you wanted...
  (best solution: Use an own ini file and load it prior to start, or let it load auto-
  matically by the command line option -useini.)

- LFE will always be mixed into l or r, if you don't give it a seperate channel. Since
  Azid.dll doesn't has the option to mix into eg. C, you have to do that manually,  if
  you want 4.0 or more precise 3/1 (l,c+LFE,r,rr+rl).


LAME:

- Certain presets of Lame DLL will overwrite/ignore other settings.
