Asterisk.org: Developer Documentation (28 Oct 2009)

Wed Oct 28 15:49:24 2009

## Asterisk developer's documentation

### - i -

- i : val
- iax_unknown : iax_ies
- ibitc : sms_s
- ibith : sms_s
- ibitl : sms_s
- ibitn : sms_s
- ibitt : sms_s
- ibytec : sms_s
- ibytep : sms_s
- ibytev : sms_s
- icard : chan_alsa_pvt
- icseq : sip_pvt
- id : sched , mgcp_subchannel , cfsip_methods , cfsip_options , skinny_device , skinny_paging_device , adsi_event , adsi_soft_key , adsi_subscript , adsi_state , dns_HEADER , adsi_flag , adsi_display , io_rec , adsi_key_cmd , ast_state_cb
- ident : rpt
- identifier : mgcp_request , ast_PGSQL_id
- identifier_type : ast_PGSQL_id
- identify : ast_imager , ast_modem_driver
- idents : ast_modem_driver
- idle : sms_s
- idtext : fast_originate_helper
- idtime : rpt
- idtimer : rpt
- ie : dundi_ie_hdr , iax2_ie , dundi_ie
- iedata : dundi_ie_hdr , ast_iax2_full_hdr
- ierr : sms_s
- ies : dundi_hdr
- ifdata : adsi_subscript
- ifinscount : adsi_subscript
- ifrn_name : my_ifreq
- ifru_addr : my_ifreq
- ignore_dtmf : chan_list
- ignored : ast_category
- ignoredtmf : zt_pvt
- ignorepats : ast_context
- ilbc : ast_filestream
- imag : sms_s
- imc0 : sms_s
- imc1 : sms_s
- immediate : mgcp_endpoint , skinny_line , zt_chan_conf , zt_pvt
- ims0 : sms_s
- ims1 : sms_s
- imsg : sms_s
- in : MD5Context
- inalarm : zt_pvt
- inbuf : mansession , skinnysession , adpcm_encoder_pvt
- include : dundi_peer
- include_level : ast_config
- includes : ast_context
- incoming_early_audio : chan_list
- incomingmsn : ast_modem_pvt
- inconference : zt_pvt
- incusecnt : ast_modem_driver
- ind : sound
- indicate : ast_channel_tech
- infd : ast_key
- info : jitterbuf
- init : ast_modem_driver
- init_v2_1 : playtones_item
- init_v2_2 : playtones_item
- init_v3_1 : playtones_item
- init_v3_2 : playtones_item
- initid : sip_pvt , chan_iax2_pvt
- initlen : adsi_soft_key
- initreq : sip_pvt
- initstr : ast_modem_pvt
- inkey : dundi_peer
- inkeys : iax2_user , iax2_peer , chan_iax2_pvt
- inlen : mansession
- inode : dlstatus
- inscount : adsi_subscript
- insmpl : ast_channel
- instance : skinny_line , select_soft_keys_message , call_info_message , register_message
- instanceNumber : buttondefinition
- interface : member_interface , member , localuser
- Intermediate_Hash : SHA1Context
- interruptible : playtones_def
- inthreeway : zt_subchannel , feature_sub
- inUse : sip_user
- inuse : ast_translator_pvt , ast_cli_entry , vpb_bridge_t
- inUse : sip_peer
- io : ast_rtp
- iobase : rpt
- iobuf : baseio
- ioc : ast_netsock , ast_netsock_list
- iocp : baseio
- ioid : ast_rtp
- iolen : baseio
- ior : io_context
- ioref : ast_netsock
- ip : register_message
- ipaddr : dundi_entity_info
- ipAddr : open_recieve_channel_ack_message
- ipc0 : sms_s
- ipc1 : sms_s
- iphasep : sms_s
- ips0 : sms_s
- ips1 : sms_s
- isAstFormat : rtpPayloadType
- iseq : mgcp_endpoint , mgcp_subchannel
- iseqno : dundi_hdr , iax_frame , ast_iax2_full_hdr , dundi_transaction , chan_iax2_pvt
- isnamedottedip : mgcp_gateway
- isremote : rpt_link
- items : playtones_def , playtones_state
- iv : dundi_encblock