Asterisk.org: Developer Documentation (28 Oct 2009)

Wed Oct 28 15:49:24 2009

## Asterisk developer's documentation

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - r -

- r_day : rule
- r_mon : rule
- r_time : rule
- r_type : rule
- r_week : rule
- ra : dns_HEADER
- radio : zt_pvt , zt_chan_conf
- randdata : sip_pvt
- random : iax2_registry , sip_registry
- rate : station_capabilities , ast_filestream
- rawdata : tdd_state , callerid_state , ast_rtp
- rawreadformat : ast_channel
- rawwriteformat : ast_channel
- rc : vpb_bridge_t
- rcode : dns_HEADER
- rd : dns_HEADER
- rdnis : oh323_pvt , sip_pvt , zt_pvt , iax_ies
- read : ast_format , ast_channel_tech , ast_custom_function , ast_modem_driver
- read_f : chan_oss_pvt
- read_filename : ast_channel_monitor
- read_image : ast_imager
- read_queue : ast_channel_spy
- read_state : vpb_pvt
- read_stream : ast_channel_monitor
- read_translator : ast_channel_spy_list
- read_vol_adjustment : ast_channel_spy
- readdata : ast_smoother
- readformat : ast_channel
- readperm : mansession
- readpos : chan_oss_pvt
- readq : ast_channel
- readthread : vpb_pvt
- readtrans : ast_channel
- realfilename : ast_filestream
- realm : sip_auth , sip_pvt , sip_registry
- realname : ast_codec_alias_table
- realtime : call_queue
- realtime_func : ast_config_engine
- realtime_multi_func : ast_config_engine
- recheck : ast_register_list
- record_gain : leave_vm_options
- record_lock : vpb_pvt
- recv : sip_pvt
- redircodecs : sip_pvt
- redirip : oh323_pvt , sip_pvt
- ref_counter : __priv_data
- refer_call : sip_pvt
- refer_contact : sip_pvt
- refer_to : sip_pvt
- reference : call_info_message , select_soft_keys_message
- referred_by : sip_pvt
- refresh : iax2_registry , sip_registry , iax_ies
- refs : dlstatus
- reg : chan_iax2_pvt , peercnt , skinny_req
- regack : skinny_req
- regattempts : sip_registry
- regex_present : refresh_info
- regexten : iax2_peer , sip_peer
- registered : skinny_device
- registerexpire : dundi_peer
- registerid : dundi_peer
- registrar : ast_exten , ast_include , ast_sw , ast_ignorepat , ast_context
- registry : sip_pvt
- regrej : skinny_req
- regstate : iax2_registry , sip_registry
- regtrans : dundi_peer
- relaxdtmf : zt_chan_conf
- release : ast_generator
- reload : module
- rem_dtmf_time : rpt
- rem_dtmfbuf : rpt
- rem_dtmfidx : rpt
- remchannel : rpt
- remid : vofr_hdr
- remmode : rpt
- remote : rpt
- remote_rr : chan_iax2_pvt
- remoteIp : start_media_transmission_message
- remoteon : rpt
- remotePort : start_media_transmission_message
- remoterx : rpt
- remotetx : rpt
- repeat : sound
- repeats : vm_state
- reportholdtime : call_queue
- reppos : playtones_def , playtones_state
- req : sip_dual
- reqeid : dundi_ies , dundi_query_state
- reqformat : local_pvt
- requester : ast_channel_tech
- res : station_capabilities , register_ack_message , soft_key_sets , skinny_req
- res2 : register_ack_message
- resched : sched
- reserved : ast_filestream
- resource : module , calloutdata
- resp : ast_rtp
- respcount : dundi_request
- response : ast_modem_pvt
- responses : mgcp_gateway
- restrictcid : zt_chan_conf , zt_pvt
- result : ast_dnsmgr_entry , enum_naptr_rr
- resync_offset : jb_info
- resync_threshold : jb_conf
- retrans : mgcp_message , sip_pkt , dundi_packet , iax_frame
- retransid : mgcp_gateway , sip_pkt , dundi_packet
- retranstimer : dundi_transaction
- retries : iax_frame , rpt_link , outgoing
- retry : call_queue
- retrydelay : osp_provider
- retrylimit : osp_provider
- retrytime : outgoing , iax_frame
- retrytimer : rpt_link
- retstr : adsi_soft_key
- retstrlen : adsi_soft_key
- retxtimer : rpt_link , rpt
- revents : pollfd
- rewrite : ast_format
- ring : distRingData
- ring_timer : vpb_pvt
- ring_timer_id : vpb_pvt
- ringback_timer : vpb_pvt
- ringback_timer_id : vpb_pvt
- ringcadence : tone_zone
- ringContext : zt_distRings
- ringerMode : set_ringer_message
- ringing : skinny_subchannel
- ringnum : zt_distRings
- rings : ast_channel
- ringt : ast_modem_pvt , zt_pvt
- ringt_base : zt_pvt
- rlPart1 : sip_request
- rlPart2 : sip_request
- rname : ast_include
- root : ast_context , ast_config , ast_category
- root_eid : dundi_request
- roundingseconds : call_queue
- route : sip_pvt
- route_persistant : sip_pvt
- row_out : dtmf_detect_state_t
- rp : sms_s , misdn_jb
- rpid : sip_pvt
- rpid_from : sip_pvt
- rprefs : chan_iax2_pvt
- rpt : rpt_tele
- rpt_call_thread : rpt
- rpt_thread : rpt
- rqnt_ident : mgcp_endpoint
- rqnt_queue : mgcp_endpoint
- rqnt_queue_lock : mgcp_endpoint
- rr_delay : iax_ies
- rr_dropped : iax_ies
- rr_jitter : iax_ies
- rr_loss : iax_ies
- rr_ooo : iax_ies
- rr_pkts : iax_ies
- rrpos : call_queue
- rsa : ast_key
- rsa_result : iax_ies
- rseqno : chan_iax2_pvt
- rtcp : ast_rtp
- rtimeout : ast_pbx
- rtp : skinny_subchannel , mgcp_subchannel , oh323_pvt , sip_pvt
- rtp_lookup_code_cache_code : ast_rtp
- rtp_lookup_code_cache_isAstFormat : ast_rtp
- rtp_lookup_code_cache_result : ast_rtp
- rtp_offered_from_local : ast_rtp
- rtpholdtimeout : sip_pvt , sip_peer
- rtpkeepalive : sip_pvt , sip_peer
- rtptimeout : sip_pvt , sip_peer
- rtype : dn_answer
- rx : sms_s
- rxchanname : rpt
- rxchannel : rpt
- rxcore : chan_iax2_pvt , ast_rtp
- rxenckey : dundi_peer
- rxflash : zt_chan_conf
- rxgain : zt_chan_conf , vpb_pvt , zt_pvt , phone_pvt
- rxpl : rpt
- rxplon : rpt
- rxseqno : ast_rtp
- rxssrc : ast_rtp
- rxswgain : vpb_pvt
- rxtrunktime : iax2_trunk_peer
- rxwink : zt_chan_conf
- rzedy : odmiana