Asterisk.org: Developer Documentation (28 Oct 2009)

Wed Oct 28 15:49:24 2009

## Asterisk developer's documentation

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - f -

- f : tonepair_state , ast_dsp , playtones_state , zt_subchannel , g726_encoder_pvt , g726_decoder_pvt , alaw_encoder_pvt , ast_translator_pvt , ulaw_decoder_pvt , ast_rtp , ulaw_encoder_pvt , ast_filestream , adpcm_encoder_pvt , ast_smoother , ast_frame_delivery , adpcm_decoder_pvt , alaw_decoder_pvt , ast_modem_pvt , g723_encoder_pvt , g723_decoder_pvt
- f_mark_idx : fsk_data
- f_space_idx : fsk_data
- fac : goertzel_state_t
- fac1 : playtones_item
- fac2 : playtones_item
- facility : logchannel
- fake : ast_translator_pvt
- fake_event : zt_pvt
- far_alerting : chan_list
- fax_hits : dtmf_detect_state_t , mf_detect_state_t
- fax_tone : dtmf_detect_state_t
- faxdetect : chan_list
- faxhandled : ast_modem_pvt , chan_list , vpb_pvt , zt_pvt
- fd : linear_state , console , ast_frame_delivery , agi_state , mansession , pollfd , ast_modem_pvt , iax_firmware , phone_pvt , skinnysession , chanspy_translation_helper , ast_conference , ast_translator_pvt
- fdcnt : io_context
- fdn : adsi_script
- fdno : ast_channel
- fds : io_context , ast_channel
- feature_mask : ast_call_feature
- feature_timer : ast_bridge_config
- features : ast_dsp
- features_callee : ast_bridge_config
- features_caller : ast_bridge_config
- filearray : mohclass
- filename : mixmonitor , ast_filestream , logchannel
- filename_base : ast_channel_monitor
- filename_changed : ast_channel_monitor
- fileptr : logchannel
- filter : refresh_info
- fin : ast_channel
- final : iax_frame
- finaldial : zt_pvt
- firmwarever : iax_ies
- first : chan_list
- first_column : yyltype , YYLTYPE
- first_line : yyltype , YYLTYPE
- firstpass : ast_bridge_config
- firstradio : zt_pvt
- fixup : ast_channel_tech
- flag : ast_app_option , ast_option_header
- flags : callerid_state , dlstatus , ast_filestream , ast_smoother , ast_rtp , ast_ivr_menu , ao2_iterator , ast_cdr , ast_channel , ast_bridge_config , mohclass , ast_channel_spy , dundi_answer , dundi_hint , dundi_peer_status , dundi_result , ast_call_feature , ast_flags , iax_template , iax2_user , iax2_peer , chan_iax2_pvt , iax2_dpcache , create_addr_info , sip_request , sip_pvt , sip_pkt , sip_user , sip_peer , vpb_bridge_t , adsi_script , localuser , mixmonitor , ast_vm_user , leave_vm_options , dundi_hint_metadata , dundi_transaction
- flags_page2 : sip_user , sip_peer
- flash : zt_chan_conf
- flashtime : zt_pvt
- flp : fsk_data
- fluffy : dundi_query_state
- flxv : fsk_data
- flyv : fsk_data
- fmp : fsk_data
- fmt : ast_filestream
- fmxv : fsk_data
- fmyv : fsk_data
- fn : vm_state , outgoing , ast_key
- fn2 : vm_state
- fname : ast_call_feature
- fo : vpb_bridge_t
- foffset : ast_filestream
- format : ast_channel_monitor , mohclass , ast_smoother , ast_channel_spy_queue , ast_imager , ast_slinfactory , iax_ies , iax_template , ast_format
- formats : ast_modem_driver , iax2_peer
- forwards : localuser
- found : create_addr_info
- fout : ast_channel
- fr : nbs_pvt , vpb_pvt , ast_modem_pvt , ast_filestream , phone_pvt
- frags : chan_oss_pvt
- frame : chan_list
- framedata : ast_smoother
- framein : ast_translator
- frameout : ast_translator
- frames : jitterbuf , station_capabilities
- frames_cur : jb_info
- frames_dropped : chan_iax2_pvt , jb_info
- frames_in : jb_info
- frames_late : jb_info
- frames_lost : jb_info
- frames_ooo : jb_info
- frames_out : jb_info
- frames_received : chan_iax2_pvt
- framesize : ast_translator_pvt
- frametype : ast_frame
- free : jitterbuf
- freq : rpt
- freq1 : tonepair_state , tonepair_def
- freq2 : tonepair_def , tonepair_state
- freqcount : ast_dsp
- freqs : ast_dsp , progress
- from : sip_pvt
- fromdomain : sip_peer , sip_pvt
- fromname : sip_pvt
- fromuser : sip_peer , sip_pvt
- fskd : tdd_state , callerid_state
- fsp : fsk_data
- fsxv : fsk_data
- fsyv : fsk_data
- fullcontact : sip_peer , sip_pvt
- fullduplex : ast_modem_driver
- fullname : ast_vm_user , cfalias
- func : ast_atexit , manager_action
- funcchar : rpt
- function : function_table_tag
- functions : rpt
- fwdata : iax_ies
- fwdatalen : iax_ies
- fwdesc : iax_ies
- fwh : iax_firmware