Asterisk.org: Developer Documentation (28 Oct 2009)

Wed Oct 28 15:49:24 2009

## Asterisk developer's documentation

# Meetme - The conference bridge configuration

- Implemented in app_meetme.c

## meetme.conf

    ;
    ; Configuration file for MeetMe simple conference rooms for Asterisk of course.
    ;
    ; This configuration file is read every time you call app meetme()

    [general]
    ;audiobuffers=32		; The number of 20ms audio buffers to be used
    				; when feeding audio frames from non-Zap channels
    				; into the conference; larger numbers will allow
    				; for the conference to 'de-jitter' audio that arrives
    				; at different timing than the conference's timing
    				; source, but can also allow for latency in hearing
    				; the audio from the speaker. Minimum value is 2,
    				; maximum value is 32.
    ;
    [rooms]
    ;
    ; Usage is conf => confno[,pin][,adminpin]
    ;
    ; Note that once a participant has called the conference, a change to the pin
    ; number done in this file will not take effect until there are no more users
    ; in the conference and it goes away.  When it is created again, it will have
    ; the new pin number.
    ;
    ;conf => 1234
    ;conf => 2345,9938