Asterisk.org: Developer Documentation (28 Oct 2009)

Wed Oct 28 15:49:24 2009

## Asterisk developer's documentation

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - d -

- da : sms_s
- data : tonepair_state , ast_smoother , fast_originate_helper , ast_db_entry , ast_iax2_video_hdr , ast_iax2_meta_trunk_hdr , ast_channel , ast_iax2_firmware_header , adsi_subscript , ast_netsock , dundi_answer , adsi_display , event_node , dundi_hint , ast_PGSQL_id , stringlink , playtones_state , ast_exten , ast_frame , dundi_packet , outgoing , ast_option_header , ast_sw , tone_zone_sound , vofr_hdr , devstate_cb , io_rec , ast_state_cb , sound , mgcp_request , app_tmp , sip_request , sip_pkt , jb_frame , ast_rtp , skinny_req , iax_frame , sched , ast_iax2_mini_hdr , ast_iax2_meta_hdr
- data_size : __priv_data
- database : ast_config_map
- datad : ast_exten
- datalen : ast_frame , sound , iax_frame , ast_iax2_firmware_header , adsi_subscript , adsi_display , dundi_packet
- dateTemplate : register_ack_message
- datetime : iax_ies
- day : definetimedate_message
- daymask : ast_timing
- dayofweek : definetimedate_message
- dbsecret : iax2_user , iax2_peer
- dcallno : iax_frame , ast_iax2_full_hdr , ast_iax2_full_enc_hdr
- dcontext : dundi_mapping , ast_cdr , dundi_request
- dcs : sms_s
- dcx : chan_iax2_pvt , dundi_transaction
- ddcomb : morse_bits
- dead : mansession , agent_pvt , iax_firmware , iax_template , member , call_queue , dundi_mapping , dundi_peer , osp_provider
- debounce : zt_chan_conf
- debug : sip_request
- dec : g723_decoder_pvt , ast_translator_pvt
- decusecnt : ast_modem_driver
- def : misdn_cfg_spec
- defaddr : iax2_peer , mgcp_gateway , sip_peer
- default_exten : ast_call_feature
- defcontext : zt_pvt
- defined : adsi_soft_key , adsi_subscript
- definetimedate : skinny_req
- definition : button_template_res_message
- dei : dundi_request
- delay : iax_rr
- deleted : vm_state
- delivery : ast_smoother , ast_frame
- delme : addr_range , mgcp_endpoint , mgcp_gateway , member , ast_key
- desc : ast_cdr_beitem , ast_cause , ast_format_list , dundi_cause , ast_imager , ast_custom_function , sound , adsi_script
- description : module , ast_app , pbx_builtin , ast_channel_tech , tone_zone , manager_action , ast_switch
- desired : volume
- dest : ast_osp_result , dundi_result , feature_pvt , dundi_mapping , outgoing
- destroy : ast_translator , zt_pvt
- destructor_fn : __priv_data
- detected_digits : dtmf_detect_state_t , mf_detect_state_t
- dev : ast_modem_pvt , phone_pvt , vpb_pvt , statechange
- device : dlstatus , skinnysession , chan_oss_pvt
- devices : skinny_paging_device
- devicestate : ast_channel_tech
- deviceStimulus : set_lamp_message
- devicetype : iax_ies
- devname : ast_iax2_firmware_header
- dial : ast_modem_driver
- dialdest : zt_pvt
- dialdigit : ast_modem_driver
- dialednone : zt_pvt
- dialing : zt_pvt
- dialledNumber : dialled_number_message
- diallednumber : skinny_req
- dialogver : sip_pvt
- dialout : ast_vm_user
- dialtimeout : ast_modem_pvt
- dialtone : phone_pvt , vpb_pvt
- dialtype : ast_modem_pvt
- didtdd : zt_pvt
- digest : ast_key
- digit_hits : dtmf_detect_state_t
- digital : zt_pvt
- digitmode : ast_dsp
- digits : dtmf_detect_state_t , mf_detect_state_t , queue_ent
- dir : mohclass
- direction : iax_frame
- directs : dundi_query_state
- disabled : logchannel
- disced : rpt_link
- disctime : rpt_link
- disgorgetime : rpt
- displayMessage : display_notify_message
- displaynotify : skinny_req
- displaypromptstatus : skinny_req
- displays : adsi_script
- displaytext : skinny_req
- displayTimeout : display_notify_message
- disposition : ast_cdr
- distinctive_ring : sip_invite_param
- distinctivering : zt_pvt
- dlcih : vofr_hdr
- dlcil : vofr_hdr
- dli_fbase : dl_info
- dli_fname : dl_info
- dli_saddr : dl_info
- dli_sname : dl_info
- dml : g726_state
- dms : g726_state
- dnd : zt_pvt , skinny_line , mgcp_endpoint
- dnid : zt_pvt , iax_ies , ast_modem_pvt , chan_iax2_pvt
- dnsmgr : iax2_peer
- domain : domain , sip_pvt , sip_registry
- dop : zt_pvt
- dowmask : ast_timing
- dpentries : chan_iax2_pvt
- dphone_functions : rpt
- dphone_longestfunc : rpt
- dproot : chan_iax2_pvt
- dpstatus : iax_ies
- dq : g726_state
- dr : dundi_request
- drings : zt_pvt
- driver : ast_config_map
- dropped : iax_rr
- dropped_frame_cnt : chan_list
- dsn : odbc_obj
- dsp : chan_list , mgcp_endpoint , zt_pvt , ast_modem_pvt
- dsp_features : zt_pvt
- dst : enum_context , ast_cdr
- dstchannel : ast_cdr
- dstfmt : ast_translator , ast_translator_pvt
- dstlen : enum_context
- dtimeout : ast_pbx
- dtmf : ast_dsp
- dtmf_caller_pos : vpb_pvt
- dtmf_time_rem : rpt
- dtmfbuf : rpt
- dtmfcount : ast_rtp
- dtmfduration : ast_rtp
- dtmff : ast_channel
- dtmfidd_timer : vpb_pvt
- dtmfidd_timer_id : vpb_pvt
- dtmfidx : rpt
- dtmfmode : mgcp_endpoint , ast_modem_pvt
- dtmfmodegen : ast_modem_pvt
- dtmfmute : ast_rtp
- dtmfq : ast_channel
- dtmfrelax : zt_pvt
- dtmfrx : ast_modem_pvt
- dtrans : dundi_hdr , dundi_transaction
- dtype : vofr_hdr
- dummy : chan_list
- dump : iax2_ie , dundi_ie
- duplex : chan_oss_pvt
- duration : tonepair_def , playtones_item , tonepair_state , ast_cdr
- dynamic : mgcp_gateway , dundi_peer , member
- dziesiatki : odmiana