Asterisk.org: Developer Documentation (28 Oct 2009)

Wed Oct 28 15:49:24 2009

## Asterisk developer's documentation

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - n -

- n_buckets : ao2_container
- name : callerid_state , ast_config_map , ast_format_list , ast_var_t , chan_oss_pvt , register_message , ast_variable , skinny_line , skinny_device , subchannel , ast_config_engine , skinny_paging_device , iax2_ie , ast_imager , iax_template , iax_flag , ast_category , ast_include , tone_zone_sound , misdn_cfg_spec , state , ast_custom_function , adsi_event , adsi_key_cmd , ast_sw , ast_switch , mixmonitor , strategy , odbc_obj , call_queue , rpt_link , ast_cdr_beitem , progalias , ast_context , ast_translator , telem_defaults , rpt , ast_modem_driver , vm_zone , dundi_ie , ast_app , agent_pvt , permission , ast_key , iax2_user , mohclass , odbc_list , ast_format , pbx_builtin , iax2_peer , osp_provider , mgcp_endpoint , ast_channel , mgcp_gateway , allowed_bearers
- naptr : enum_naptr_rr
- naptr_rrs : enum_context
- naptr_rrs_count : enum_context
- naptrinput : enum_context
- nastki : odmiana
- nat : skinny_subchannel , ast_rtp , mgcp_subchannel
- nativeformats : ast_channel , oh323_pvt
- nbit : fsk_data
- nbs : nbs_pvt
- need_busy : chan_list
- need_hangup : chan_list
- need_queue_hangup : chan_list
- need_rtp : cfsip_methods
- needanswer : zt_subchannel
- needaudit : mgcp_endpoint
- needbusy : zt_subchannel
- needcallerid : zt_subchannel
- needcongestion : zt_subchannel
- needdestroy : oh323_pvt , mgcp_endpoint , skinny_line
- needflash : zt_subchannel
- needhangup : oh323_pvt
- needringing : zt_subchannel
- needsgain : ast_filestream
- needshrink : io_context
- netaddr : ast_ha
- netlag : dundi_peer_status
- netmask : ast_ha
- newcontrol : oh323_pvt
- newmessages : vm_state
- newpvt : ast_translator
- newstate : oh323_pvt
- next : mgcp_gateway , skinnysession , queue_ent , mgcp_message , ast_filestream , ast_variable , ast_config_engine , iax2_registry , iax_firmware , ast_frame , ast_imager , iax2_user , tone_zone_sound , tone_zone , eventqent , agent_pvt , mansession , member , rpt_tele , manager_action , ast_custom_function , ast_switch , ast_rtp_protocol , ast_translator , ast_modem_driver , ast_modem_pvt , vpb_pvt , state , feature_pvt , oh323_pvt , iax2_context , ast_cli_entry , iax2_peer , ast_cdr , ast_db_entry , agi_command , ast_ha , ast_trans_pvt , iax2_trunk_peer , sched , localuser , ast_state_cb , zt_pvt , ast_context , ast_ignorepat , iax2_dpcache , local_pvt , ast_exten , mgcp_request , mgcp_response , mgcp_subchannel , logchannel , mgcp_endpoint , skinny_device , chan_list , jb_frame , robin_list , enum_search , mohclass , ast_category , dundi_request , dundi_precache_queue , chan_oss_pvt , ast_cdr_batch_item , vm_zone , ast_atexit , sip_route , sip_history , sip_auth , msn_list , sip_pvt , sip_pkt , skinny_subchannel , skinny_line , skinny_paging_device , phone_pvt , iax_frame , iax_template , event_node , call_queue , rpt_link , asent , ast_vm_user , chanlist , permission , dundi_packet , ast_config_map , ast_comment , dlstatus , parkeduser , ast_format , module , loadupdate , msglist , verb , ast_channel , dundi_peer , dundi_mapping , ast_frame_delivery , ast_hint , ast_app , mohdata , subchannel , channel , osp_provider , ast_include , ast_sw , dundi_transaction , stringlink , ast_key , fillin
- next_flag : ast_filestream , adpcm_state , g726_encoder_pvt
- next_voice_ts : jb_info
- nextin : ast_trans_pvt
- nextout : ast_trans_pvt
- nextpred : chan_iax2_pvt
- nitems : playtones_def , playtones_state
- noautorespond_on_setup : chan_list
- nobusyout : rpt
- nocache : dundi_query_state
- nodes : rpt
- nonce : sip_pvt , sip_registry
- noncecount : sip_pvt , sip_registry
- nonCodecCapability : oh323_pvt
- noncodeccapability : sip_pvt
- nonCodecCapability : skinny_line , mgcp_endpoint
- nooptimization : local_pvt
- norxtone : chan_list
- nosound : chan_oss_pvt
- notquiteyet : parkeduser
- notsilenttx : chan_iax2_pvt
- notxtone : chan_list
- npos : playtones_state
- nrringcadence : tone_zone
- nscount : dns_HEADER
- nstop : fsk_data
- nttimeout : chan_list
- num : misdn_cfg_pt , permalias
- num_buttons : button_defs
- number : dundi_request , callerid_state , dundi_precache_queue
- numbufs : zt_chan_conf
- numdisplays : adsi_script
- numflags : adsi_script
- numkeys : adsi_script
- nummaps : dundi_query_state
- numresults : ast_osp_result
- numstates : adsi_script
- numsubs : adsi_script