Asterisk.org: Developer Documentation (28 Oct 2009)

Wed Oct 28 15:49:24 2009

## Asterisk developer's documentation

# MGCP configuration

Also see RTP configuration RTP configuration

- Implemented in chan_mgcp.c

## mgcp.conf

    ;
    ; MGCP Configuration for Asterisk
    ;
    [general]
    ;port = 2427
    ;bindaddr = 0.0.0.0

    ;[dlinkgw]
    ;host = 192.168.0.64
    ;context = default
    ;canreinvite = no
    ;line => aaln/2
    ;line => aaln/1

    ;; The MGCP channel supports the following service codes:
    ;; # - Transfer
    ;; *67 - Calling Number Delivery Blocking
    ;; *70 - Cancel Call Waiting
    ;; *72 - Call Forwarding Activation
    ;; *73 - Call Forwarding Deactivation
    ;; *78 - Do Not Disturb Activation
    ;; *79 - Do Not Disturb Deactivation
    ;; *8 - Call pick-up
    ;
    ; known to work with Swissvoice IP10s
    ;[192.168.1.20]
    ;context=local
    ;host=192.168.1.20
    ;callerid = "John Doe" <123>
    ;callgroup=0      ; in the range from 0 to 63
    ;pickupgroup=0    ; in the range from 0 to 63
    ;nat=no
    ;threewaycalling=yes
    ;transfer=yes     ; transfer requires threewaycalling=yes. Use FLASH to transfer
    ;callwaiting=yes  ; this might be a cause of trouble for ip10s
    ;cancallforward=yes
    ;line => aaln/1
    ;

    ;[dph100]
    ;
    ; Supporting the DPH100M requires defining DLINK_BUGGY_FIRMWARE in
    ; chan_mgcp.c in addition to enabling the slowsequence mode due to
    ; bugs in the D-Link firmware
    ;
    ;context=local
    ;host=dynamic
    ;dtmfmode=none		; DTMF Mode can be 'none', 'rfc2833', or 'inband' or
    				; 'hybrid' which starts in none and moves to inband.  Default is none.
    ;slowsequence=yes	; The DPH100M does not follow MGCP standards for sequencing
    ;line => aaln/1

    ; known to work with wave7optics FTTH LMGs
    ;[192.168.1.20]
    ;accountcode	= 1000		; record this in cdr as account identification for billing
    ;amaflags	= billing	; record this in cdr as flagged for 'billing', 'documentation', or 'omit'
    ;context	= local
    ;host		= 192.168.1.20
    ;wcardep	= aaln/*	; enables wildcard endpoint and sets it to 'aaln/*' another common format is '*'
    ;callerid 	= "Duane Cox" <123>	; now lets setup line 1 using per endpoint configuration...
    ;callwaiting	= no
    ;callreturn	= yes
    ;cancallforward = yes
    ;canreinvite	= no
    ;transfer	= no
    ;dtmfmode	= inband
    ;line => aaln/1			; now lets save this config to line1 aka aaln/1
    ;callerid 	= "Duane Cox" <456>	; now lets setup line 2
    ;callwaiting	= no
    ;callreturn	= yes
    ;cancallforward = yes
    ;canreinvite	= no
    ;transfer	= no
    ;dtmfmode	= inband
    ;line => aaln/2			; now lets save this config to line2 aka aaln/2